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Installation Tips

LEAF RACEWEAR ( lap belts, shoulder harnesses and crotch belts meet or exceed the SFI 16.1 specification.  Useful life of the webbing should not exceed two years and it is recommended that they be replaced at or before that time.

If involved in an accident or the webbing or hardware shows wear or abuse, return to the manufacturer for inspection or replacement.  All hardware on lap belt, harness and anti-submarine crotch belts are not to be welded on, bent or straightened, as this will cause fracture.

( All mounting brackets must be installed at an angle that is compatible with the direction of the pull on the webbing under full load.

( Mounting brackets must be attached directly to the frame or chassis.  Do not mount to sheet metal or floorboards.

( Seat belts should be anchored apart, the width of the driver.

( Seat belts should be anchored at a 45-degree angle to the floor.  

See drawing.

( Anti-submarine belts should be anchored behind the chest line.

( Always use Grade 8 bolts, nuts and washers for driver restraint installations. 

( All hardware used to manufacture these driver restraints are manufactured in sheet alloy steel and drop forged alloy steel.

( All labels and tags should not be positioned under adjusters or slider bars. 
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NOTE:

Hardware on the ends of the lap belt that attaches your belt assembly to the floor area must be mounted in a vertical position. Shoulder harnesses and lap belts must be mounted vertically.
WARNING

These articles are sold without warranty, expressed or implied.  No warranty or representation is made to these products ability to protect the user from any injury or death.  Be advised that automobile racing and other forms of motorsports are dangerous and products are subject to failure when exposed to the high stress that is involved.  The user assumes that risk and all responsibilities.

Leaf Racewear & Safety Equipment Inc.
